Prosoft Technology Inc
README FILE FOR MVI56(E)-MNET SAMPLE LADDER PROGRAMS
Date: 2/20/14

OVERVIEW

"Add-On version 1.4 considers data block 0 (read and write) as containing the first data block. 
Block 0 is only generated when a maximum of one block is configured. 
This feature was introduced in version 2.05.000. 

Added the support of Block 9990/9991 which is to Set and Get the IP address of the module.  

Version 1.5 status data is updated for Block ID's between -1 and 25 only.

Version 1.61 resolves minor arithmetic overflow fault when msb of WriteData registers are set during a function 5 or 15 while passthru is enabled

This zip file MVI56E_MNET SAMPLE LADDERS.zip contains the following files: 

MVI56(E)MNET_AddOn_Rung_v1_5.L5X - Import rung file for RSLogix v16 or later
MVI56EMNET_Optional_AddOn_Rung_v1_0.L5X - Optional rung file
MVI56EMNET_v20.ACD - Sample ladder program for RSLogix v20 (with Add-On instruction). 
MVI56EMNET_v19.ACD - Sample ladder program for RSLogix v19 (with Add-On instruction). 
MVI56EMNET_v18.ACD - Sample ladder program for RSLogix v18 (with Add-On instruction). 
MVI56EMNET_v17.ACD - Sample ladder program for RSLogix v17 (with Add-On instruction). 
MVI56EMNET_v16.ACD - Sample ladder program for RSLogix v16 (with Add-On instruction).   
MVI56EMNET_v15.ACD - Sample ladder program for RSLogix v15. 
MVI56EMNET_v13.ACD - Sample ladder program for RSLogix v13.     

README.TXT - Readme file (this file)  


SELECTING THE LADDER FILE

>For CompactLogix version 16.xx.xx or later

RSLogix version 16 introduced the Add-On instruction funcionality that allows
the encapsulation of several ladder rungs into one single instruction. The sample 
ladder logic for v16 uses the Add-On instruction in order to provide a quick and easy
setup procedure for your MVI56-MNET module.
You can either import the required components into your existing ladder through the 
MVI56(E)MNET_AddOn_Rung_v1_5.L5X file or refer to the sample ladder file MVI56MNET_v16.ACD. 

In order import the required components into your existing ladder program follow
the steps below:  

1) Create a new RSLogix project for version 16 or later

2) Create a new module 1756-MODULE (I/O Configuration) with the following settings: 

Name                            = MVI56MNET
Comm Format                     = Data-INT
Input Assembly Instance         = 1
Input Assembly Size             = 250
Output Assembly Instance        = 2
Output Assembly Size            = 248
Configuration Assembly Instance = 4

Adjust the Slot and RPI settings(if enabled) for your application.

Note - recommended RPI time is 5.0ms for local rack applications. 

3) Write-click at the rung where the Add-On instruction will be inserted.
Select Import Rung... and select the MVI56(E)MNET_AddOn_Rung_v1_5.L5X file.  During the import 
procedure associate the input and output images with the ones generated 
during step 1 (default are for slot 1). 

4) Once the import procedure is completed the Add-On instruction will be 
displayed at the ladder rung. The procedure has also imported new User-Defined Data types
and New Controller tags. 

5) Verify the project 

6) Save the project

7) Download the project to the ControlLogix processor


You can also refer to the sample ladder MVI56_MNET_v16.ACD or later that already 
contains the complete project with the Add-On instruction and module created 
with correct settings.

>For ControlLogix version 13.xx.xx

Refer to the sample ladder logic MVI56EMNET_v13.ACD


USING THE SAMPLE LADDER FILE

For information on how to access the sample program controller tags please refer
to the MVI56E-MNET USer Manual. 

